PRE-START Canopy LOCKED Park Brake ON Circuit breakers CHECK Master Switch ON Fuel Switch LOWEST TANK Throttle IDLE Propeller FULL FINE Avionics OFF Fuel pump ON Fuel Pressure Warn CK OFF Fuel pump OFF Choke if cold engine ON “Clear Prop” ANNOUNCE Starter ENGAGE AFTER START Oil Pressure >1.5 BAR Choke OFF Throttle 820 RPM Avionics ON SYMBOLS Δ Difference | OR & AND ± Range of plus or minus ≤ Less than or equal to ≥ Greater than or equal to	RUN-UP Oil Temp ≥50°C Park Brake ON Choke OFF Fuel FULLEST TANK Throttle 1700 RPM Ign R/L ≤120 RPM Δ ≤50 RPM Propeller CYCLE x3 Propeller Δ 200±50RPM Carburettor heat ON→OFF Idle CHECK ≥580 RPM Throttle SET 820 RPM PRE TAKE-OFF Trim SET TKOF Mixture CHOKE OFF Prop Pitch FULL FINE Flight CTRL FREE&CORRECT Flaps TKOF 17° Fuel FULLEST TANK&PUMP ON Instruments CHECK Switches CIRC BRKERS Switches AS REQ Hatches & Harnesses CHECK Safety/DEP BRIEF HOLDING READY Lights STROBE ON Camera XPDR 3000 ALT Action READY, REQ CLR	PRE LANDING Brakes PRESSURE&OFF Undercarriage DOWN&LOCKED Mixture CHOKE OFF Fuel SUFF QTY & PUMP ON Instruments CHECK Switches AS REQ Hatches & Harnesses CHECK AFTER LANDING Lights OFF Flaps & Trim SET TKOF SHUT DOWN Park Brake ON Throttle MIN RPM Avionics OFF Ignition RIGHT ...pause 2 seconds Ignition OFF Master Switch OFF AFTER SHUT DOWN MR if last FLT of day CLOSE Hobbs/Tach REC BOOK Hobbs/Tach REC OFFICE Aircraft SECURE&CLEAN
EMERG FORCED LDG Aviate, Navigate, Comm. Best Glide 78KIAS Troubleshoot F.A.S.T. Fuel pump ON Fuel select CHANGE CHECK Air CARB HEAT ON Switches IGNITION BOTH Switches MASTER ON Throttle CYCLE Turn over ENGINE START Field SELECT Wind Obstacles Size Shape Surface Slope Sun Shoots Surroundings/Buildings Communicate MAYDAY Passenger BRIEF Aircraft SECURE	STALL ENTRY Clearing Turn AS REQ Height RECOVER ≥3000 AGL Aircraft CONFIG, TRIM Security HARNESS, OBJECTS Engine OPS NORMAL, P/T Location UNPOPUL, FLD AVBL Lookout TRAFFIC Listen CHECK FREQ SPEEDS Vne 165KIAS Vno 130KIAS Va 112KIAS Vfe 90KIAS Vs0 39KIAS Vs1 49KIAS Vx 52KIAS Vy 65KIAS Best Glide 78KIAS Max crosswind 15KT	FREQUENCIES YBAF ATIS 120.90MHz YBAF SMC 119.90MHz YBAF TWR (NORTH) 123.60MHz YBAF TWR (SOUTH) 118.10MHz YBAF CTAF 118.10MHz YBAF AWIS 128.40MHz YBAF PAL 118.10MHz BN CEN Train. 125.70MHz BN CEN 45NM N. 129.00MHz BN CEN 14NM S. 119.50MHz YHEC CTAF 119.00MHz Southport CTAF 119.00MHz YAMB ATIS 123.30MHz GEN Air Distress 121.50MHz ENGINE Model Rotax 912ULS Max RPM (cont.) 2260RPM Block Fuel Burn 24L/hr Min VFR Reserve 45min Fuel 95RON|AVGAS100LL Min Oil Temp 50°C Max Oil QTY 3.0L Min Oil QTY 2.55L
	VH-BNE Total Fuel Capacity 120.0L Total Fuel Capacity 86.4kg Total Usable Fuel 109.6L Total Usable Fuel 78.9kg Basic Empty Weight 521.4kg Max Take-Off Weight 750kg Usable Load at full fuel 149.7kg Empty Arm 434.0mm Permitted CG min. 427mm Permitted CG max. 523mm Min Crew Weight 54.9kg Max Baggage Weight 40kg Max LF (no flaps) +4G Min LF (no flaps) -2G Max LF (flaps) +2G Min LF (flaps) 0G Max Angle of Bank 60° Propeller MTV-21-A/175-05 ⌀1750mm Primary Flight Display Garmin G500 Maximum propeller speed 2260RPM Flap positions 0° 17° 35°
Aquila A210 Quick Reference Checklist
Document Metadata	Aquila A210 Checklist
hosted at: https://system-f.gitlab.io/documentation/miscellaneous
source hosted at: https://gitlab.com/system-f/documentation/miscellaneous
last updated at time: 2025-11-21 04:13:34 UTC by Tony Morris <tonymorris@gmail.com>
revision: 04f62baa9b6349a20e84923537d48f4f1ef6d4a0	Page 3 of 3
access control: public