PRE-START Pre-flight CMPL Park Brake ON Beacon light ON Avionics OFF Circuit Breakers CHECK Autopilot OFF Cowl Flaps OPEN Fuel Selector !BOTH Throttle Friction SET If engine is COLD, prime Fuel Primer STROKE x3 Carburettor Heat OFF Throttle ∙10mm OPEN Np ∙FULL FINE Fuel Mixture ∙FULL RICH Propeller Area CHECK “Clear Prop” ANNOUNCE Master Switch ON Starter ENGAGE AFTER START Oil Pressure 30-100psi Throttle ∙1000 RPM Fuel Mixture ∙LEAN Avionics ON NAV Lights ON Transponder SDBY Flaps VERIFY/RETRACT Cockpit config CFM	RUN-UP Fuel Mixture ∙FULL RICH Park Brake ON Throttle ∙1700 RPM Ignition R CHECK ≤150 RPM Ignition L CHECK ≤150 RPM Ignition R/L Δ ≤50 RPM Carb Heat ON→OFF(RPM drop) Vacuum Gauge CHECK Np ∙CYCLE Alt. Static CHECK Idle CHECK ≥600 RPM Autopilot CHECK PRE TAKE-OFF T rim SET TKOF M ixture ∙FULL RICH P rop Pitch ∙FULL FINE F light CTRL FREE,CORRECT F laps SET TKOF 10° F uel !BOTH,QTY,PRIMER LOCK I nstruments CHECK S witches AS REQ H atches & H arnesses SECURE T/O Safety/DEP/TEM !BRIEF HOLDING READY Lights STROBE ON Camera XPDR 3000 ALT Action READY, REQ CLR	PRE LANDING B rakes PRESSURE&OFF U ndercarriage !DOWN&LOCKED M ixture ∙RICH F uel !SELECT BOTH,SUFF QTY I nstruments CHECK S witches AS REQ H atches & H arnesses CHECK AFTER LANDING Carburettor Heat OFF Flaps RETRACT 0° Cowl Flaps OPEN Transponder SDBY Fuel Mixture ∙LEAN Landing Light OFF SHUT DOWN Park Brake ON Trim SET TKOF Throttle ∙MIN RPM Avionics OFF Fuel Mixture ∙IDLE CUTOFF Magnetos OFF Master Switch OFF AFTER SHUT DOWN MR if last FLT of day CLOSE Hobbs/Tach REC BOOK Hobbs/Tach REC OFFICE Aircraft SECURE
EMERG FORCED LDG Aviate, Navigate, Comm. Best Glide 70KIAS Troubleshoot F.A.S.T. F uel primer LOCKED F uel selector BOTH A ir CARB HEAT ON S witches ON T hrottle CYCLE T urn over ENGINE START Field SELECT W ind O bstacles S ize S hape S urface S lope S un S hoots S urroundings/Buildings Communicate MAYDAY Passenger BRIEF Aircraft SECURE	STALL ENTRY Clearing Turn AS REQ H eight RECOVER ≥3000 AGL A ircraft CONFIG, TRIM S ecurity HARNESS, OBJECTS E ngine OPS NORMAL, P/T L ocation UNPOPUL, FLD AVBL L ookout TRAFFIC L isten CHECK FREQ SPEEDS & LIMITS Vne 176KIAS Vno 141KIAS Va2950lb 110KIAS Va2450lb 100KIAS Va1950lb 89KIAS Vfe0-10° 140KIAS Vfe10-40° 95KIAS Vs0 48KIAS Vs1 53KIAS Vx 59KIAS Vy 80KIAS Best Glide 70KIAS Max crosswindlanding 20KT Max crosswindtakeoff 15KT Load Factorcruise +3.8G/-1.52G Load Factorflaps +2.0G Angle of Bank 60° Service Ceiling 17700ft	FREQUENCIES YBAF ATIS 120.90MHz YBAF SMC 119.90MHz YBAF TWR (NORTH) 123.60MHz YBAF TWR (SOUTH) 118.10MHz YBAF CTAF 118.10MHz YBAF AWIS 128.40MHz YBAF PAL 118.10MHz BN CEN Train. 125.70MHz BN CEN 45NM N. 129.00MHz BN CEN 14NM S. 119.50MHz YHEC CTAF 119.00MHz YAMB ATIS 123.30MHz GEN Air Distress 121.50MHz ENGINE & FUEL Model Continental 6cyl Max Power 230BHP@2600RPM Max RPM 2600RPM Block Fuel Burn 55L/hr Min VFR Reserve 30min Total Fuel 80.0USG/303.0L Usable Fuel 75.0USG/285.0L Fuel Type AVGAS100LL Max Oil Temp 116°C/460°F Min Oil QTY 9QT/8.5L Max Oil QTY 12QT/11.3L Min Oil Pressure 10psi Max Oil Pressure 100psi
VH-TIN
WEIGHT & BALANCE MTOW 2950 lb MTOW 1338.1 kg MLW 2950 lb MLW 1338.1 kg Max load@full fuel 664.9 lb Max load@full fuel 301.72 kg Max Area A 120 lb Max Area A 54.55 kg Max Area B+hatshelf 80 lb Max Area B+hatshelf 36.36 kg Max hatshelf 25 lb Max hatshelf 11.36 kg BEW 1835.1 lb BEW 832.38 kg Arm 36.5 in Arm 926 mm Moment 66908 lb/in Moment 770892 kg/mm MTOW 2950lb example Row 1 160 kg Row 2 160 kg Area A (max) 54.55 kg Area B (max) 36.36 kg Fuel 94.81 kg 131.68 L 34.86 USG	CRUISE PERFORMANCE 75% power 65% power 55% power Altitude KTAS NM/L KTAS NM/L KTAS NM/L 3000 140 2.63 132 2.89 122 3.11 6500 144 2.74 136 3.00 125 3.18 10000 140 3.08 128 3.26 Standard conditions, nil wind ISA-20 temp (-13°C) ISA temp (7°C) ISA+20 temp (27°C) RPM MP %BHP KTAS L/hr %BHP KTAS L/hr %BHP KTAS L/hr 2450 23 77 142 54.0 74 143 52.1 22 75 138 53.2 73 139 50.9 70 140 49.4 21 71 135 49.8 69 136 48.3 66 137 46.7 20 67 132 47.1 65 133 45.2 62 133 44.1 2400 23 78 139 55.1 75 141 52.8 72 142 50.9 22 74 137 51.7 71 138 49.8 69 139 48.3 21 70 134 49.0 67 135 47.1 65 136 45.6 20 66 131 46.0 63 132 44.5 61 132 43.3 2300 23 74 137 51.7 71 138 49.8 69 139 48.3 22 70 134 49.1 67 135 47.5 65 136 46.0 21 66 131 46.4 64 132 44.8 62 133 43.3 20 62 128 43.7 60 128 42.2 58 128 41.0 Pressure Altitude 4000ft @ 2950lb
Cessna 182P Quick Reference Checklist
Document Metadata	Cessna 182P Checklist
hosted at: https://system-f.gitlab.io/documentation/miscellaneous
source hosted at: https://gitlab.com/system-f/documentation/miscellaneous
last updated at time: 2025-11-21 04:13:34 UTC by Tony Morris <tonymorris@gmail.com>
revision: 04f62baa9b6349a20e84923537d48f4f1ef6d4a0	Page 3 of 3
access control: public