PRE-START Park Brake ON Circuit Breakers CHECK Master Switch KEY ENGINE Choke if cold engine ON Fuel Pump ON→PRESSURE Fuel Pump OFF Throttle MIN + ½ TURN Ignition 1 & 2 ON Propeller Area CHECK “Clear Prop” ANNOUNCE Starter ENGAGE AFTER START Oil Pressure RISING/GREEN Choke OFF Throttle 2000 RPM Avionics ON SYMBOLS Δ Difference | OR & AND ≤ Less than or equal to ≥ Greater than or equal to	RUN-UP Oil Temp ≥50°C Park Brake ON Choke OFF Throttle 3600 RPM Ignition 1 CHECK ≤125 RPM Ignition 2 CHECK ≤125 RPM Ignition 1/2 Δ ≤50 RPM Carburettor Heat ON→OFF Idle CHECK ≥1250 RPM Throttle 2000 RPM PRE TAKE-OFF Trim SET TKOF Mixture CHOKE OFF Prop Pitch FULL FINE Flight CTRL FREE&CORRECT Flaps SET TKOF Fuel ON&SUFF QTY Instruments CHECK Switches AS REQ Hatches & Harnesses CHECK T/O Safety/DEP/TEM BRIEF HOLDING READY Lights STROBE ON Camera XPDR 3000 ALT Action READY, REQ CLR	PRE LANDING Brakes PRESSURE&OFF Undercarriage DOWN&LOCKED Mixture CHOKE OFF Fuel ON&SUFF QTY Instruments CHECK Switches AS REQ Hatches & Harnesses CHECK AFTER LANDING Lights OFF Flaps & Trim SET TKOF SHUT DOWN Park Brake ON Flaps & Trim SET TKOF Throttle MIN RPM Avionics OFF Ignition 1 OFF ...pause 2 seconds Ignition 2 OFF Master Switch KEY OFF AFTER SHUT DOWN MR if last FLT of day CLOSE Hobbs/Tach REC BOOK Hobbs/Tach REC OFFICE Aircraft SECURE
EMERG FORCED LDG Aviate, Navigate, Comm. Best Glide 65KIAS Troubleshoot F.A.S.T. Fuel pump ON Fuel selectors 3xON Air CARB HEAT ON Switches IGNITION 2xON Switches MASTER ON Throttle CYCLE Turn over ENGINE START Field SELECT Wind Obstacles Size Shape Surface Slope Sun Shoots Surroundings/Buildings Communicate MAYDAY Passenger BRIEF Aircraft SECURE	STALL ENTRY Clearing Turn AS REQ Height RECOVER ≥2000 AGL Aircraft CONFIG, TRIM Security HARNESS, OBJECTS Engine OPS NORMAL, P/T Location UNPOPUL, FLD AVBL Lookout TRAFFIC Listen CHECK FREQ SPEEDS Vne 124KIAS Va 95KIAS Vfe 81KIAS Vs0 36KIAS Vs1 43KIAS Vx 60KIAS Vy 65KIAS Best Glide 65KIAS Max wind (RWY HDG) 25KT Max crosswind 15KT Max tailwind 6KT	FREQUENCIES YBAF ATIS 120.90MHz YBAF SMC 119.90MHz YBAF TWR (NORTH) 123.60MHz YBAF TWR (SOUTH) 118.10MHz YBAF CTAF 118.10MHz YBAF AWIS 128.40MHz YBAF PAL 118.10MHz BN CEN Train. 125.70MHz BN CEN 45NM N. 129.00MHz BN CEN 14NM S. 119.50MHz YHEC CTAF 119.00MHz Southport CTAF 119.00MHz YAMB ATIS 123.30MHz GEN Air Distress 121.50MHz ENGINE Model Rotax 912ULS Max RPM (5 mins) 5800RPM Max RPM (cont.) 5500RPM Block Fuel Burn 20L/hr Min VFR Reserve 45min Fuel 95RON|AVGAS100LL Min Oil Temp 50°C Max Oil QTY 2.6L Min Oil QTY 2.1L
24-4844 Total Fuel Capacity 85.1L Total Fuel Capacity 61.3kg Total Usable Fuel 83L Total Usable Fuel 59.8kg Basic Empty Weight 288.5kg Empty Arm 244.8mm Empty Arm 18.83% Permitted CG min. 259.08mm Permitted CG min. 20% Permitted CG max. 363.22mm Permitted CG max. 28% Max Take-Off Weight 560kg Min Crew Weight 55kg Max Baggage Weight 20kg Max LF (no flaps) +4G Min LF (no flaps) -2G Max LF (flaps) +2G Min LF (flaps) 0G Max Angle of Bank 60° Max endurance 6 hours Max range 534NM Service ceiling 14760ft Propeller FITI ECO ⌀1580mm	24-5350 Total Fuel Capacity 85.0L Total Fuel Capacity 61.2kg Total Usable Fuel 83L Total Usable Fuel 59.8kg Basic Empty Weight 303.5kg Empty Arm 266.0mm Empty Arm 20.46% Permitted CG min. 259.08mm Permitted CG min. 20% Permitted CG max. 363.22mm Permitted CG max. 28% Max Take-Off Weight 560kg Min Crew Weight 54.9kg Max Baggage Weight 20kg Max LF (no flaps) +4G Min LF (no flaps) -2G Max LF (flaps) +2G Min LF (flaps) 0G Max Angle of Bank 60° Max endurance 6 hours Max range 534NM Service ceiling 14760ft Propeller FITI ECO ⌀1580mm	24-8881 Total Fuel Capacity 86.0L Total Fuel Capacity 61.9kg Total Usable Fuel 85L Total Usable Fuel 61.2kg Basic Empty Weight 303.8kg Empty Arm 304.0mm Empty Arm 24.18% Permitted CG min. 260mm Permitted CG min. 20% Permitted CG max. 442mm Permitted CG max. 34% Max Take-Off Weight 560kg Min Crew Weight 54kg Max Baggage Weight 20kg Max LF (no flaps) +4G Min LF (no flaps) -2G Max LF (flaps) +2G Min LF (flaps) 0G Max Angle of Bank 60° Max endurance 6 hours Max range 534NM Service ceiling 14760ft Propeller FITI ECO ⌀1580mm
Eurofox 3K Quick Reference Checklist
Document Metadata	Eurofox 3K Checklist
hosted at: https://system-f.gitlab.io/documentation/miscellaneous
source hosted at: https://gitlab.com/system-f/documentation/miscellaneous
last updated at time: 2025-11-21 04:13:34 UTC by Tony Morris <tonymorris@gmail.com>
revision: 04f62baa9b6349a20e84923537d48f4f1ef6d4a0	Page 3 of 3
access control: public