PRE-START Park Brake ON Battery Isolator OFF Master Switch ON Throttle IDLE Fuel Pumps A+B ON Lane A+B ON Start Switch HOLD UP Lane A/B Lights Check OFF Propeller Area CHECK “Clear Prop” ANNOUNCE Start Button PRESS AFTER START Oil Pressure RISING/GREEN Throttle 2000 RPM Avionics ON SYMBOLS Δ Difference | OR & AND ≤ Less than or equal to ≥ Greater than or equal to	RUN-UP Oil Temp ≥50°C Park Brake ON Throttle 3000 RPM Battery Charge CHECK ON Idle CHECK ≥1400 RPM Throttle 2000 RPM PRE TAKE-OFF Trim SET TKOF Mixture CHOKE OFF Prop Pitch FULL FINE Flight CTRL FREE&CORRECT Flaps SET TKOF Fuel ON&SUFF QTY Instruments CHECK Switches AS REQ Hatches & Harnesses CHECK Safety/DEP BRIEF HOLDING READY Lights STROBE ON Camera XPDR 3000 ALT Action READY, REQ CLR	PRE LANDING Brakes PRESSURE&OFF Undercarriage DOWN&LOCKED Mixture N/A Fuel ON&SUFF QTY Instruments CHECK Switches AS REQ Hatches & Harnesses CHECK AFTER LANDING Lights OFF Flaps & Trim SET TKOF SHUT DOWN Park Brake ON Flaps & Trim SET TKOF Throttle IDLE Avionics OFF Fuel Pumps A/B OFF Lane A OFF Lane B OFF Master Switch KEY OFF Battery Isolator ON AFTER SHUT DOWN MR if last FLT of day CLOSE Hobbs/Tach REC BOOK Hobbs/Tach REC OFFICE Aircraft SECURE
EMERG FORCED LDG Aviate, Navigate, Comm. Best Glide 54 KIAS Troubleshoot F.A.S.T. Fuel Pumps ON Fuel selectors ON Air Alternate Switches LANEs A/B ON Switches MASTER ON Throttle CYCLE Turn over ENGINE START Field SELECT Wind Obstacles Size Shape Surface Slope Sun Shoots Surroundings/Buildings Communicate MAYDAY Passenger BRIEF Aircraft SECURE	STALL ENTRY Clearing Turn AS REQ Height RECOVER ≥2000 AGL Aircraft CONFIG, TRIM Security HARNESS, OBJECTS Engine OPS NORMAL, P/T Location UNPOPUL, FLD AVBL Lookout TRAFFIC Listen CHECK FREQ SPEEDS Vne 124KIAS Va 101KIAS Vfe 80KIAS Vs0 32KIAS Vs1 42KIAS Vx 46KIAS Vy 52KIAS Best Glide 54KIAS Max crosswind 14KTS	FREQUENCIES YBAF ATIS 120.90MHz YBAF SMC 119.90MHz YBAF TWR (NORTH) 123.60MHz YBAF TWR (SOUTH) 118.10MHz YBAF CTAF 118.10MHz YBAF AWIS 128.40MHz YBAF PAL 118.10MHz BN CEN Train. 125.70MHz BN CEN 45NM N. 129.00MHz BN CEN 14NM S. 119.50MHz YHEC CTAF 119.00MHz Southport CTAF 119.00MHz YAMB ATIS 123.30MHz GEN Air Distress 121.50MHz ENGINE Model Rotax 912ULS Max RPM (5 mins) 5800RPM Max RPM (cont.) 5500RPM Block Fuel Burn 20L/hr Min VFR Reserve 45min Fuel 95RON|AVGAS100LL Min Oil Temp 50°C Max Oil QTY 2.6L Min Oil QTY 2.1L
Foxbat A22LS Quick Reference Checklist
Document Metadata	Foxbat A22LS Checklist
hosted at: https://system-f.gitlab.io/documentation/miscellaneous
source hosted at: https://gitlab.com/system-f/documentation/miscellaneous
last updated at time: 2025-11-21 04:13:34 UTC by Tony Morris <tonymorris@gmail.com>
revision: 04f62baa9b6349a20e84923537d48f4f1ef6d4a0	Page 2 of 2
access control: public