COLD START Fuel Mixture ∙FULL RICH Master Switch ON Alternator ON Fuel Pump ON Throttle ∙⅛ OPEN Fuel Pump OFF Propeller Pitch ∙FULL FINE Flaps RETRACT 0° “Clear Prop” ANNOUNCE Starter ENGAGE WARM START Fuel Mixture ∙LEAN Throttle ∙⅛ OPEN Propeller Pitch ∙FULL FINE Master Switch ON Alternator ON Flaps RETRACT 0° “Clear Prop” ANNOUNCE Starter ENGAGE Fuel Mixture ∙FULL RICH AFTER START Oil Pressure IDLE @ 25psi Fuel Mixture ∙LEAN Avionics ON NAV Lights ON Transponder SDBY Flaps VERIFY/RETRACT Cockpit config CFM RUN-UP Fuel Mixture ∙FULL RICH Park Brake ON Throttle ∙1700 RPM Ignition R CHECK ≤50 RPM Ignition L CHECK ≤50 RPM Np ∙CYCLE Idle CHECK ≥600 RPM Autopilot CHECK T.M.P.F.I.S.H.	SPEEDS & LIMITS Vne 200KIAS Vno 156KIAS Va 130KIAS Vfe 100KIAS Vs0 51KIAS Vs1 62KIAS Vx 70KIAS Vy 95KIAS Best Glide 78KIAS Service Ceiling 19500ft AEROBATICS Loop, Horiz. Eight 122-165KIAS Immelman Turn 130-165KIAS Aileron/Barrel Roll 105-165KIAS Snap Roll 70-95KIAS Vertical Roll 156-165KIAS Split-S 87-96KIAS ENGINE & FUEL Model Superior IO-400 Block Fuel Burn 40L/hr Min VFR Reserve 30min Total Fuel 188.0L Fuel Type AVGAS100LL Max Oil Temp 118°C/245°F Min Oil QTY 2QT/1.9L Max Oil QTY 8QT/7.6L Min oper. Oil Pressure 55psi Max oper. Oil Pressure 95psi WEIGHT & BALANCE MTOW 930 kg BEW 579 kg Arm 2068.0 mm Moment 1196757 kg/mm Full Fuel (188L) 135.36 kg Max load@full fuel 215.64 kg Max Baggage 45.4 kg Crew Arm 2536.0 mm Fuel Arm 2082.0 mm Baggage Arm 3288.8 mm CG Limit 2084.8-2241.3 mm
Vans RV-14 Quick Reference Checklist
Document Metadata	Vans RV-14 Checklist
hosted at: https://system-f.gitlab.io/documentation/miscellaneous
source hosted at: https://gitlab.com/system-f/documentation/miscellaneous
last updated at time: 2025-11-21 04:13:34 UTC by Tony Morris <tonymorris@gmail.com>
revision: 04f62baa9b6349a20e84923537d48f4f1ef6d4a0	Page 1 of 1
access control: public